**[Ausschreibungstext](http://www.ausschreiben.de/online/usr/show.php?tb=richter_kunststofftechnik&ade=0&showtree=1&ids=8&tbframe=richter_kunststofftechnik" \o "Ausschreibungstext einblenden bzw. ausblenden)**

**GreenLife Kellertank 1.000 l / GKT 1.25**

Volumen: 1.000 l

Mögliche Anschlussgrößen: DN 32 – DN 110 (Sondergrößen auf Anfrage)

Einstiegsöffnung: 550 mm

Farbe: anthrazit

Material: hergestellt aus Polyethylen (physiologisch unbedenklich)

Der Kellertank 1.000 l / GKT 1.25 ist für die oberirdische Aufstellung bzw. im Gebäude / Innenbereich geeignet.

Kellertank aus Polyethylen (PE), hergestellt im Rotationssinterverfahren (nahtlos und spannungsfrei in einem Stück gefertigt), UV-Beständig und lichtundurchlässig, weitere Montageflächen an allen Seiten mit diverse Anschlussmöglichkeiten für Untenverbindungen.

Mögliche Anschlussgrößen: DN 110

10 Jahre Materialgarantie auf den Behälter!

Hohe Formstabilität durch dicke Wandstärken mit zusätzlicher 6-facher Stahl-Profil-Versteifung

UV-Beständigkeit für konstante Materialqualität.

Optionale Ausstattungsvarianten erhältlich z.B. Zulaufberuhiger, Überlaufsiphon, als Hybridmanager / Trennstation

 Material: Polyethylen, Stahlversteifungen

Inhalt: 1.000 l

Gewicht: 60 kg

Länge: 1.240 mm

Breite: 720 mm

Höhe: 1.595 mm

Artikelnummer: G0000719

Mengeneinheit: Stück

Herstellerangaben:

GreenLife GmbH

Sacktannen 1a

19057 Schwerin

Telefon +49 (0) 385 – 77337-0

Telefax +49 (0) 385 – 77337-33

Web www.greenlife.de

E-Mail projects@greenlife.info

Menge: ………… Einheit: **Stk**. EP: ………… GP: …………

**tender specifications**

**GreenLife basement tank 1.000 l / GKT 1.25**

volume: 1.000 l

possible connection sizes: DN 32 – DN 110 (special sizes on request)

manhole: 550 mm

colour: anthracite

material: made of polyethylene (physiologically harmless)

The basement tank 1.000 l / GKT 1.25 is suitable for installation above ground or in the building / indoors.

Basement tank made of polyethylene (PE), manufactured in a rotation sintering process (seamless and stress-free in one piece), UV-resistant and light-proof, additional mounting surfaces on all sides with various connection options for bottom connections.

possible connection sizes: DN 110

10 years material guarantee on the tank!

High dimensional stability due to thick walls with additional 6-fold steel profile reinforcement

UV resistance for constant material quality.

Optional equipment variants available e.g. calmed inlet, overflow siphon, as hybrid manager / separation station

material: polyethylene, steel profiles

volume: 1.000 l

weight: 60 kg

length: 1.240 mm

width: 720 mm

height: 1.595 mm

item no: G0000719

unit of quantity: piece

manufacturer:

GreenLife GmbH

Sacktannen 1a

D-19057 Schwerin

Germany

phone +49 (0) 385 – 77337-0

web www.greenlife.de

e-mail projects@greenlife.info

quantity: ………… unit: **piece** single price: ………… total price: …………