**[Ausschreibungstext](http://www.ausschreiben.de/online/usr/show.php?tb=richter_kunststofftechnik&ade=0&showtree=1&ids=8&tbframe=richter_kunststofftechnik" \o "Ausschreibungstext einblenden bzw. ausblenden)**

**GreenLife Sickerschacht** **950 l**

inkl. Kunststoffabdeckung (begehbar)

im Vergleich zu Beton einfacheres Handling – geringeres Gewicht

Sickerschacht mit Kunststoffabdeckung, (optional: frei ablängbar zur Geländeanpassung),

mit eingehängtem Grobschmutzfilterkorb (befestig mit Kunststoffkette)

Anschluss: per Gummilippendichtung DN 100

(diverse Anschlussmöglichkeiten frei wählbar mit Gummilippendichtungen von DN 32 - DN 100)

Einstiegsöffnung 600 mm (gemäß DIN 1989) – zur Inspektion

inkl. Sicherheitskunststoffabdeckung 200 kg begehbar,

Kindersicher verschraubbar mit 2 Edelstahlschrauben

Option: PKW-befahrbar (bis 600 kg Achslast) – PKW-BefahrbarkeitsSet (G0001724)

LKW-befahrbar (SLW 40) – Set LKW-Befahrbarkeit (G0003335)

Optionale Ausstattungsvarianten erhältlich!

15 Jahre Materialgarantie auf den Behälter!

Hohe Formstabilität durch dicke Wandstärken

UV-Beständigkeit für konstante Materialqualität.

Gewicht: 58 kg

Material: PE

Durchmesser: 762 / 800 mm

Höhe: 2.150 mm

Artikelnummer: G0003701

Mengeneinheit: Stück

Herstellerangaben:

GreenLife GmbH

Sacktannen 1a

19057 Schwerin

Telefon +49 (0) 385 – 77337-0

Telefax +49 (0) 385 – 77337-33

Web www.greenlife.de

E-Mail projects@greenlife.info

Menge: ………… Einheit: **Stk**. EP: ………… GP: …………

[**tender**](http://www.ausschreiben.de/online/usr/show.php?tb=richter_kunststofftechnik&ade=0&showtree=1&ids=8&tbframe=richter_kunststofftechnik) **specifications**

**GreenLife percolation shaft** **950 l**

incl. plastic cover (walkable)

easier handling in comparison to concrete shafts – lower weight

percolation shaft with plastic cover (optionally: can be cutted to adjust to the terrain surface),

with mounted coarse filter basket (fixed with plastic chain)

connection: with rubber gasket DN 100

(diverse connection options – free to choose with rubber gaskets from DN 32 - DN 100)

access opening 600 mm (according DIN 1989) – for inspection purposes

incl. plastic safety cover (load capacity: 200 kg, walkable),

child-safe screwed – with 2 stainless steel screws

option: accessible by cars (up to 600 kg axle load) – Kit accessible by cars (G0001724)

accessibility for trucks (class D) - kit for accessibility of trucks (G0003335)

Optional equipment versions available!

15 years material warranty on the tanks/shafts!

Strong walls – best construction of GreenLife stability profiles

UV resistance for a constant material quality

weight: 58 kg

material: PE

diameter: 762 / 800 mm

height: 2.150 mm

item no.: G0003701

unit of quantity: piece

manufacturer:

GreenLife GmbH

Sacktannen 1a

D-19057 Schwerin

Germany

phone +49 (0) 385 – 77337-0

fax +49 (0) 385 – 77337-33

web www.greenlife.de

e-mail projects@greenlife.info

quantity: ………… unit: **piece** single price: ………… total price: …………