**[Ausschreibungstext](http://www.ausschreiben.de/online/usr/show.php?tb=richter_kunststofftechnik&ade=0&showtree=1&ids=8&tbframe=richter_kunststofftechnik" \o "Ausschreibungstext einblenden bzw. ausblenden)**

**GreenLife Sickerflachtank 5.000 l**

inkl. Kunststoffabdeckung (begehbar)

Rückhaltevolumen: 5.000 l

Mögliche Anschlussgrößen: DN 100/110

inkl. Ausgleichsdom 380 mm – 580 mm stufenlos ausziehbar und

bis 5° neigbar zur optimalen Geländeanpassung

Einstiegsöffnung 600 mm (gemäß DIN 1989) – zur Inspektion

inkl. Sicherheitskunststoffabdeckung 200 kg begehbar,

Kindersicher verschraubbar mit 2 Edelstahlschrauben

Optionen: PKW-befahrbar (bis 600 kg Radlast) – Set für PKW-Befahrbarkeit (G0001724)

im Vergleich zu Beton einfacheres Handling – geringeres Gewicht

Flachtank aus Polyethylen (PE), hergestellt im Rotationssinterverfahren, hohe Formstabilität durch patentiertes Stabilitätsdesign, UV-Beständig und lichtundurchlässig, mit aufgesetztem Ausgleichsdom DN 600 mm, Domschacht stufenlos einstellbar, weitere Montageflächen an allen Seiten mit diverse Anschlussmöglichkeiten. Optional mit Filter.

Der Sickerflachtank 5000 l eignet sich für die Rückhaltung, Versickerung und Entwässerung von Regenwasser. Der Zulauf in den Sickerflachtank ist mit einer Gummilippendichtung DN 100 vorbereitet. Der Sickerflachtank ist einfach zu warten, inspizieren und reinigen.

15 Jahre Materialgarantie auf den Behälter!

Hohe Formstabilität durch dicke Wandstärken

UV-Beständigkeit für konstante Materialqualität.

Inhalt: 5.000 l

Gewicht: 210 kg

Material: PE

Länge: 2.420 mm

Breite: 2.200 mm

Höhe mit Dom: 1.440 – 1.640 mm

Artikelnummer: G0006214

Mengeneinheit: Stück

Herstellerangaben:

GreenLife GmbH

Sacktannen 1a

19057 Schwerin

Telefon +49 (0) 385 – 77337-0

Telefax +49 (0) 385 – 77337-33

Web www.greenlife.de

E-Mail projects@greenlife.info

Menge: ………… Einheit: **Stk**. EP: ………… GP: …………

[**tender**](http://www.ausschreiben.de/online/usr/show.php?tb=richter_kunststofftechnik&ade=0&showtree=1&ids=8&tbframe=richter_kunststofftechnik) **specifications**

**GreenLife percolation flat tank 5000 l**

volume: 5000 l

possible connection sizes: DN 100/110

incl. sliding dome 380 – 580 mm infinitely extendable and 5° tilt for optimized adaptation to terrain surface

access opening 600 mm (according DIN 1989) – for inspection purposes

incl. plastic safety cover (load capacity: 200 kg, walkable),

child-safe screwed – with 2 stainless steel screws

options: accessible by cars (up to 600 kg wheel load) – Kit accessible by cars (G0001724)

easier handling in comparison to concrete shafts – lower weight

Percolation flat tank made of polyethylene (PE), produced in rotation sintering method, high dimensional stability due to patented stability design, UV-resistant and impervious to light, with attached sliding dome DN 600 mm manhole continuously adjustable, 3 connections DN 100 for supply and overflow, and supply line, additional mounting surfaces on all sides with several interfaces. Optional with filter.

The 5000 l percolation flat tank is suitable for the retention, infiltration and drainage of rainwater. The inlet to the percolation flat tank is prepared with a DN 100 rubber lip seal. The percolation flat tank is easy to maintain, inspect and clean.

15 years material warranty on the tanks/shafts!

strong walls – best construction of GreenLife stability profiles

UV resistance for a constant material quality

volume: 5000 l

weight: 210 kg

material: PE

length: 2420 mm

diameter: 2200 mm

height: 1440 – 1640 mm

item no.: G0006214

unit of quantity: piece

manufacturer:

GreenLife GmbH

Sacktannen 1a

D-19057 Schwerin

Germany

phone +49 (0) 385 – 77337-0

fax +49 (0) 385 – 77337-33

web www.greenlife.de

e-mail projects@greenlife.info

quantity: ………… unit: **piece** single price: ………… total price: …………